=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=
 __  __   ______   ______   ______       __    __   ______    
/\ \_\ \ /\  ___\ /\  == \ /\  __ \     /\ "-./  \ /\  ___\   
\ \  __ \\ \  __\ \ \  __< \ \ \/\ \    \ \ \-./\ \\ \  __\   
 \ \_\ \_\\ \_____\\ \_\ \_\\ \_____\    \ \_\ \ \_\\ \_____\ 
  \/_/\/_/ \/_____/ \/_/ /_/ \/_____/     \/_/  \/_/ \/_____/ 
 ______   __  __   __   __       _____    ______   ______     
/\  == \ /\ \/\ \ /\ \ /\ \     /\  __-. /\  ___\ /\  == \    
\ \  __< \ \ \_\ \\ \ \\ \ \____\ \ \/\ \\ \  __\ \ \  __<    
 \ \_____\\ \_____\\ \_\\ \_____\\ \____- \ \_____\\ \_\ \_\  
  \/_____/ \/_____/ \/_/ \/_____/ \/____/  \/_____/ \/_/ /_/  
                                                              
=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

Thank you for using the Hero Me Builder! 

Most parts are interchangeable, however some are too unique to be compatible with the Builder. For example, the Anycubic Chiron uses a gantry adapter that attaches to the probe mounts instead of the back of the base.
A lot of spacers and niche parts are also not compatible with the Builder because they are modeled together in a single stl and cannot be seperated.
Please consult the full Hero Me Gen 7 zip to see if any parts are required for your specific setup but not listed. https://www.printables.com/model/39322-hero-me-gen7-platform-release4 
Help is also available through the Hero Me Community Discord, join us at https://discord.gg/QHKqQrvzZv 

Report issues, or offer your own Hero Me community parts to be added, to support@heromebuilder.com